PERMANENT PRESERVATIVE TREATMENT CERTIFICATE

Unique identifiable link to the consignment:

Description of goods/packaging treated:
(such as pallets and crates if packaging is treated)

Quantity/volume of goods/packaging treated:

Date of treatment:

Name of preservative formulation

Chemical class of preservative (active ingredients)

Retention of active ingredient (loading of preservative) expressed as

 % mass/mass based on the oven dried mass of the treated wood; or mass per volume (net dry salt retention – Fenvalerate and Fenitrothion ONLY).

NOTE: %mass/mass = 100 x actual batch retention of active ingredient in penetration zone (mass/vol) actual oven dried mass of the treated wood (mass/vol)

**Plywood, LVL and veneers only:**

Veneer only treatment[ ]  or glue line only treatment[ ]  or both [ ] (please tick one)

Veneer thickness [ ] mm or [ ] inches

**STATEMENT (tick one box):**

[ ]  This is to certify that the timber described below was treated in accordance with Department of Agriculture, Fisheries and Forestry biosecurity penetration and retention requirements with an acceptable (listed) preservative formulation.

[ ]  This is to certify that the timber described below was treated in accordance with Australian Standard® AS/NZS1604 to specific Department of Agriculture, Fisheries and Forestry biosecurity penetration and retention requirements.

Additional statements as required by the import conditions for the relevant goods/packaging (if applicable)

Signature: Printed name:

(Company employee) (Employee name)

Date of issue:

 (DD/MM/YYYY)